Light Imperial-class Repulsortank
Name/Model# : | Imperial Repulsortank 1-L (Light Imperial-class Repulsortank)
Designer/Manufacturer : | Ubrikkian Transports
Combat Designation : | Light Repulsortank
Scale : | Speeder
Length : | 20.5 Metres
Skill : | Repulsorlift operation: Imperial-class Repulsortank
Crew Skill : | Repulsorlift operation 5D+2 and vehicle blasters 5D+2
Crew : | 2 (Driver and Gunner)
Troops : | 2 Troops/Passengers
Cost of Vehicle : | 40,000 Credits
Vehicle Speed : | 300 kph (WEG=105)
Altitude Range : | 2 Metres from Ground Level
Manoeuvrability : | 1D+2
Cargo Capacity : | 300 kg
Weapons : | 1 Turreted Medium Blaster Cannon Crew: 1 Gunner Fire Control: 1D+1 Range: 50 metres-200 metres/500 metres/1 km Damage: 3D+2
Cover of Vehicle : | Full
Shields/Body Strength : | Shields None. Body Strength 4D+2
The Light Imperial-class Repulsortank shares the same medium-range chassis employed by the Medium and Heavy Imperial-class Repulsortanks. Its classification like the other two repulsortanks in the series is derived from the craft's armament. It is an economical version of the heavy repulsortank minus the expensive heavy gun intended primarily for a garrison tank. The 1-L is usually crewed by regular troops under the tight command of their sergeant via comlink. A passenger seat is maintained for use by the section sergeant or platoon sergeant major, both of whom traditionally shift vehicles from day to day.
Sources: AJ9***Pg 228, 229
[Main][Back]