Medium Imperial-class Repulsortank
Name/Model# : | Imperial Repulsortank 1-M (Medium Imperial-class Repulsortank)
Designer/Manufacturer : | Ubrikkian Transports
Combat Designation : | Medium Repulsortank
Scale : | Speeder
Length : | 20.5 Metres
Skill : | Repulsorlift operation: Imperial-class Repulsortank
Crew Skill : | Repulsorlift operation 5D+2 and vehicle blasters 5D+2
Crew : | 3 Crew 1 + Gunners 2
Troops : | 3 Troops/Passengers
Cost of Vehicle : | 45,000 Credits
Vehicle Speed : | 300 kph (WEG=105)
Altitude Range : | 2 Metres from Ground Level
Manoeuvrability : | 1D+2
Cargo Capacity : | 250 kg
Weapons : | 1 Turreted Medium Blaster Cannon Crew: 1 Gunner Fire Control: 1D+1 Range: 50 metres-200 metres/500 metres/1 km Damage: 3D+2 1 Turreted Heavy Repeating Blaster (Can face Forward / Left / Right Arcs Only) Crew: 1 Gunner Scale: Character Fire Control: 1D+1 Range: 3-75/200/500 metres Damage: 8D
Cover of Vehicle : | Full
Shields/Body Strength : | Shields None. Body Strength 4D+2
The Medium Imperial-class Repulsortank is a limited production command vehicle, which are employed by platoon officers in the field to keep close command on their units. Its secondary weapon, an anti-personnel heavy repeating blaster allows protection against ground troops, while not allowing officers to seek out maverick engagements. The 1-M features enough space for the driver, gunner, lieutenant and sergeant major, and the communications equipment necessary for the command of the armour unit. When compared to the 1-L and the 1-H, the 1-M has more room and crew space. The M-1 is the basic model of the Imperial-class Repulsortank. The main heavy gun was replaced with a command and control seat for the commanding officer. These craft are assigned the medium designation since they lack the armament of a heavy repulsortank, and officers do not ride in light repulsortanks.
Sources: AJ9***Pg 222, 230, 231
[Main][Back]